Altera's SoCFPGA platform device tree bindings
---------------------------------------------

Boards with Cyclone 5 SoC:
Required root node properties:
compatible = "altr,socfpga-cyclone5", "altr,socfpga";

Boards with Arria 5 SoC:
Required root node properties:
compatible = "altr,socfpga-arria5", "altr,socfpga";

Boards with Arria 10 SoC:
Required root node properties:
compatible = "altr,socfpga-arria10", "altr,socfpga";
