Analog TV Connector
===================

Required properties:
- compatible: "composite-video-connector" or "svideo-connector"

Optional properties:
- label: a symbolic name for the connector

Required nodes:
- Video port for TV input

Example
-------

tv: connector {
	compatible = "composite-video-connector";
	label = "tv";

	port {
		tv_connector_in: endpoint {
			remote-endpoint = <&venc_out>;
		};
	};
};
