MOXA ART device tree bindings

Boards with the MOXA ART SoC shall have the following properties:

Required root node property:

compatible = "moxa,moxart";

Boards:

- UC-7112-LX: embedded computer
  compatible = "moxa,moxart-uc-7112-lx", "moxa,moxart"
