* Cirrus Logic CLPS711X Timer Counter

Required properties:
- compatible: Shall contain "cirrus,clps711x-timer".
- reg       : Address and length of the register set.
- interrupts: The interrupt number of the timer.
- clocks    : phandle of timer reference clock.

Note: Each timer should have an alias correctly numbered in "aliases" node.

Example:
	aliases {
		timer0 = &timer1;
		timer1 = &timer2;
	};

	timer1: timer@80000300 {
		compatible = "cirrus,ep7312-timer", "cirrus,clps711x-timer";
		reg = <0x80000300 0x4>;
		interrupts = <8>;
		clocks = <&clks 5>;
	};

	timer2: timer@80000340 {
		compatible = "cirrus,ep7312-timer", "cirrus,clps711x-timer";
		reg = <0x80000340 0x4>;
		interrupts = <9>;
		clocks = <&clks 6>;
	};
