MediaTek mt65xx & mt81xx Platforms Device Tree Bindings

Boards with a MediaTek mt65xx/mt81xx SoC shall have the following property:

Required root node property:

compatible: Must contain one of
   "mediatek,mt6589"
   "mediatek,mt6592"
   "mediatek,mt8127"
   "mediatek,mt8135"
   "mediatek,mt8173"


Supported boards:

- bq Aquaris5 smart phone:
    Required root node properties:
      - compatible = "mundoreader,bq-aquaris5", "mediatek,mt6589";
- Evaluation board for MT6592:
    Required root node properties:
      - compatible = "mediatek,mt6592-evb", "mediatek,mt6592";
- MTK mt8127 tablet moose EVB:
    Required root node properties:
      - compatible = "mediatek,mt8127-moose", "mediatek,mt8127";
- MTK mt8135 tablet EVB:
    Required root node properties:
      - compatible = "mediatek,mt8135-evbp1", "mediatek,mt8135";
- MTK mt8173 tablet EVB:
    Required root node properties:
      - compatible = "mediatek,mt8173-evb", "mediatek,mt8173";
