NVIDIA Tegra Flow Controller

Required properties:
- compatible: Should be "nvidia,tegra<chip>-flowctrl"
- reg: Should contain one register range (address and length)

Example:

	flow-controller@60007000 {
		compatible = "nvidia,tegra20-flowctrl";
		reg = <0x60007000 0x1000>;
	};
